###4.16.16 (26.06.18)

**New features:**

- 18.8 stable firmware for Galileosky 7 and Galileosky Base Block is added.
- 231.23 stable firmware for Galileosky GLONASS/GPS is added.

**Change log of 18.8 firmware:**

	Corrections:
	1) Error in sychronization with WebDAV is fixed.
	2) Error in Easy Logic commands parser is fixed.
	3) SIM cards switching error is fixed.

**Change log of 231.23 firmware:**
    Сorrections:
    1) Error during SMS parsing is fixed.	
	
###4.16.13 (14.06.18)

**New features:**

- 18.7 stable firmware for Galileosky Base Block is added.

**Change log of 18.7 firmware:**

	Corrections:
	1) Data send error is fixed.

###4.16.12 (13.06.18)

**New features:**

- 18.6 stable firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 18.6 firmware:**

	New features:
	1) Ability to set up prohibited GSM networks is added.
	Corrections:
	1) Error during synchronization with WebDAV server is fixed.

###4.16.11 (16.03.18)

**New features:**

- 231.22 stable firmware for Galileosky GLONASS/GPS is added.
- 18.4 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 18.4 firmware:**
    New features:
    1) Collected archive data retransmission through GSM is added.
    2) Better WebDAV support.
    Сorrections:
    1) Incoming SMS parsing error is fixed.
    2) Encryption in Galileosky protocol is fixed.

**Change log of 231.22 firmware:**
    Сorrections:
    1) Error during SMS parsing is fixed.

###4.16.10 (20.02.18)

**New features:**

- 18.3 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 18.3 firmware:**
    Сorrections:
    1) Error of setting impulses to zero in the Easy Logic tab is fixed.

###4.16.9 (07.02.18)

**New features:**

- 18.2 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Corrections:**

- Algorithm uploading error is fixed.

**Change log of 18.2 firmware:**
    Сorrections:
    1) Ability to switch Wi-Fi unit working mode using Easy Logic is added.

###4.16.8 (02.02.18)

**New features:**

- 18.1 beta firmware for Galileosky 7 is added.

**Change log of 18.1 firmware:**
    Сorrections:
    1) FLS data transmission error is fixed.

###4.16.7 (07.12.17)

**New features:**

- 231.21 stable firmware for Galileosky GLONASS/GPS is added.
- 17.5 beta firmware for Galileosky 7 and Galileosky Base Block is added.
- 18.0 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 231.21 firmware:**
    Corrections:
    1) Autoinformer files parsing error is fixed.

**Change log of 17.5 firmware:**
    New features:
    1) GSMINFO command is added.
    Сorrections:
    1) FLS values are set to zero after disconnection.
    2) Error during remote downloading of Easy Logic algorithms is fixed.

**Change log of 18.0 firmware:**
    Сorrections:
    1) Driver behaviour detection algorithm is changed. It uses now accelerometer measurements.
    2) Archive collection from other devices using Wi-Fi is added. (For Galileosky Base Block only)
    
###4.16.6 (21.11.17)

**New features:**

- 17.4 beta firmware for Galileosky 7 and Galileosky Base Block is added.
- 231.20 stable firmware for Galileosky GLONASS/GPS is added.

**Change log of 17.4 firmware:**
    Сorrections:
    1) Easy Logic algorithms startup error is fixed.

**Change log of 231.20 firmware:**
    Corrections:
    1) Defrost detection error with EuroScan is fixed.

###4.16.5 (14.11.17)

**New features:**

- 17.3 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 17.3 firmware:**
    Сorrections:
    1) CAN initialization error is fixed.

###4.16.4 (03.11.17)

**New features:**

- 17.2 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Corrections:**

- A rare crash during application startup is fixed. Device orientation widget is temporary disabled.

**Change log of 17.2 firmware:**
    New features:
    1) Possibility to send commands to the tracking unit by means of Easy Logic is added. Only those commands are supported that do not modify the settings of the tracking unit.
    Сorrections:
    1) SD card initialization error is fixed.
    2) Better WebDAV compatibility.
    3) Shock and tilt detection error is fixed.

###4.16.3 (30.10.17)

**New features:**

- 17.1 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 17.1 firmware:**
    New features:
    1) SIM-card priority is added.
    2) Inputs state is accessible in Easy Logic.
    3) FLS data in EGTS protocol is added. Archive structure is changed, all unsent data will be lost.
    Сorrections:
    1) CAN initialisation error in Easy Logic is fixed.
    2) Better WebDAV compatibility.

###4.16.2 (30.10.17)

**New features:**

- 16.7 stable firmware for Galileosky 7 is added.
- Sending FLS data with addresses 3-15 from the file of internal memory archive to the server is added.
- Ability to edit simultaneously several calibration tables is added.

**Change log of 16.7 firmware:**
    Corrections:
    1) GSM power on is fixed.

###4.16.1 (24.10.17)

**Corrections:**

- Wrong main packet setup is fixed.

###4.16.0 (25.09.17)

**New features:**

- 16.6 stable firmware for Galileosky 7 and Galileosky Base Block is added.
- 17.0 beta firmware for Galileosky 7 and Galileosky Base Block is added.
- 231.18 stable firmware for Galileosky GLONASS/GPS is added.

**Change log of 16.6 firmware:**
    New features:
    1) GNSS module data absence indication is added.
    Corrections:
    1) Error during registartion in GSM network is fixed.
    2) Error in Wiegand26 handler is fixed.
    3) Arguments substitution in command responses from EasyLogic is added.

**Change log of 17.0 firmware:**
    New features:
    1) Ability to syncronize data stored on SD card with WebDAV server is added.
    2) A filtering and transforning mechanism for measured data is added. 
    3) Mileage setup commnad is added.
    4) Multiple EasyLogic algorithms could be run simultaneously.

**Change log of 231.18 firmware:**
    Corrections:
    1) Error in CAN-LOG handler is fixed.

###4.15.3 (13.09.17)

**New features:**

- 16.4 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 16.4 firmware:**

    Corrections:
    1) GSM module power off from EasyLogic is fixed.

###4.15.2 (31.08.17)

**New features:**

- 231.17 stable firmware for Galileosky GLONASS/GPS is added.
- 16.3 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 231.17 firmware:**

    Corrections:
    1) Error in responses to CAN filters setup commands is fixed.

**Change log of 16.3 firmware:**

    Corrections:
    1) First packet is sent after connection drop.
    2) Ringer sound level is increased.

###4.15.1 (26.08.17)

**New features:**

- 229.18 and 231.16 stable firmwares for Galileosky GLONASS/GPS are added.
- 16.2 beta firmware for Galileosky 7 and Galileosky Base Block is added.

**Change log of 229.18 firmware:**

    Corrections:
    1) After accumulator discharge internal time is set to 01/01/2000.

**Change log of 231.16 firmware:**

    Corrections:
    1) Error with saving RS485 FLS temperature using EasyLogic is fixed.

###4.15.0 (25.08.17)

**New features:**

- Portuguese version of the Configurator is prepared. 

###4.14.8 (24.08.17)

**New features:**

- 16.1 beta firmware for Galileosky 7 is added.

**Change log of 16.1 firmware:**

    Corrections:
    1) Mistake concerning frequent breaks of server connection via Wi-Fi is fixed.

###4.14.7 (18.08.17)

**New features:**

- Spanish version of the Configurator is prepared. 
- 16.0 beta firmware for Galileosky 7 is added.

**Change log of 16.0 firmware:**

    Corrections:
    1) Wrong refrigerator data transmission is fixed.

###4.14.6 (09.08.17)

**New features:**

- 15.7 beta firmware for Galileosky Base Block is added.

**Change log of 15.7 firmware:**

    Corrections:
    1) Better photo read errors handling.

###4.14.4 (03.08.17)

**New features:**

- 231.15 stable firmware for Galileosky GLONASS/GPS are added.

**Change log of 231.15 firmware:**

    New features:
    1) Reply to incorrect SMS with russian symbols is disabled.
    Corrections:
    1) Error with geofences recording is fixed. 

###4.14.3 (31.07.17)

**New features:**

- 15.6 beta firmware for Galileosky Base Block is added.

**Change log of 15.6 firmware:**

    New features:
    1) Maximum speed filtration is added. Command gps.correct is not compatible with 1.x firmwares.
    Corrections:
    1) External power detection is fixed.
    2) Removing old photos from SD card is fixed

###4.14.2 (31.07.17)

**New features:**

- 2.0 beta firmware for Galileosky 7 is added.

**Change log of 2.0 firmware for Galileosky 7**

    New features:
    1) Signaling mode is added.
    2) Ability to store trusted keys on SD card is added.
    3) Receiving CAN messages in EasyLogic is added.
    4) Sending CAN messages from EasyLogic is added.
    5) Remote config is enabled by default.
    6) Maximum speed filtration is added. Command gps.correct is not compatible with 1.x firmwares.
    Corrections:
    1) Better frequency measurement accuracy.

###4.14.1 (26.07.17)

**New features:**

- 15.5 beta firmware for Galileosky Base Block is added.
- 231.14 and 229.17 stable firmwares for Galileosky GLONASS/GPS are added.

**Change log of 15.5 firmware:**

    New features:
    1) DataCOLD600 and Carrier Gateway support.
    2) Request RPM data from DataCOLD500. Archive structure has been changed, all saved data will be lost.

**Change log of 231.14 and 229.17 firmwares:**

    Corrections:
    1) Error, connected with CAN data reset to zero while operating in OBDII mode, is fixed.

###4.14.0 (24.07.17)

**New features:**

- 15.4 beta firmware for Galileosky Base Block is added.

**Change log of 15.4 firmware for Galileosky Base Block:**

    Corrections:
    1) Wrong transmission of PressurePro data is fixed.
    2) Wrong transmission of fridge data is fixed.
    3) Wrong transmission of photos is fixed.
    4) Mileage data is accessible from EasyLogic.

###4.13.10 (17.07.17)

**New features:**

- 1.6 beta firmware for Galileosky 7 is added.

**Change log of 1.6 firmware for Galileosky 7**

    Corrections:
    1) Power on of GSM is fixed.

###4.13.9 (14.07.17)

**New features:**

- 1.5 beta firmware for Galileosky 7 is added.
- IN 4 and IN5 could be set as ignition sensors for Galileosky 7.

**Change log of 1.5 firmware for Galileosky 7**

    Corrections:
    1) Wrong measurements on IN4 and IN5 are fixed.
    2) Setup commands for SIM1 are added.

###4.13.8 (29.06.17)

**New features:**

- 16 RS485 FLS are shown on "Device" tab.

###4.13.6 (19.06.17)

**New features:**

- 15.1 beta firmware for Galileosky Base Block is added.


**Change log of 15.1 firmware for Galileosky Base Block:**

    New features:
    1) Signaling mode is added.
    2) Ability to store trusted keys on SD card is added.
    Corrections:
    1) Faster switching to SIM-chip if preferred GSM-networks are set.

###4.13.5 (16.06.17)

**New features:**

- 231.13 stable firmware for GALILEOSKY GLONASS/GPS v5.1, v5.0, v4.0, v2.5, v2.5 lite is added.

**Change log of 231.13 firmware:**

    Corrections:
    1) Error in microphone gain setup on terminals with SIM900 is fixed.
    2) Reset during setup is fixed.
    3) Out of order message is sent using Iridium modem if connection with server is not available.

###4.13.3 (23.05.17)

**New features:**

- 14.5 beta firmware for Galileosky Base Block is added.

**Change log of 14.5 firmware for Galileosky Boxfinder:**

    Corrections:
    1) Error in archive with chronological send order is fixed.
    2) Error in settings for SIM-chip is fixed.

###4.13.2 (22.05.17)

**New features:**

- 10 stable firmware for Galileosky Boxfinder is added.

**Change log of 10 firmware for Galileosky Boxfinder:**

    Corrections:
    1) Archive handling error is fixed.

###4.12.33 (07.04.17)

**New features:**

- 12.10 stable firmware and 14.1 beta firmware for GALILEOSKY Base Block are added.

**Change log of 12.10 firmware:**

    Corrections:
    1) Error of detection of GLONASS aerial connection is fixed.

**Change log of 14.1 firmware:**

    New features:
    1) Time syncronization using GSM.
    2) Inputs values set blocks and impulse count shutdown blocks in EasyLogic are implemented.
    Corrections:
    1) Sending photo error is fixed.
    2) iButton handling error is fixed.
    3) Wrong coordinates fitering by external power is fixed.

###4.12.32 (03.04.17)

**New features:**

- 231.8 beta firmware for GALILEOSKY GLONASS/GPS v5.1, v5.0, v4.0, v2.5, v2.5 lite is added.

**Change log of firmware:**

    New features:
    1) DataCOLD600 support.
    Corrections:
    1) Internal time is set to 01.01.2000 after accumulator discharge.

###4.12.31 (10.03.17)

**New features:**

- 231.7 beta firmware for GALILEOSKY GLONASS/GPS v5.1, v5.0, v4.0, v2.5, v2.5 lite is added.

**Change log of firmware:**

    Corrections:
    1) Error in roaming handling with SIM800 is fixed.
    2) Machine hours request from EruroScan is fixed.

###4.12.30 (03.03.17)
 
 **New features:**
 
- 229.15 stable firmware and 231.5 beta firmware for GALILEOSKY GLONASS/GPS v5.1, v5.0, v4.0, v2.5, v2.5 lite are added.
 
**Change log of firmwares:**
 
     Corrections:
    1) Coordinates filtering error is fixed.

###4.12.29 (02.03.17)

**New features:**

- Wi-Fi control functions are added to EasyLogic.

###4.12.28 (16.02.17)

**New features:**

- 14 beta firmware for GALILEOSKY Base Block is added.
- 231.5 beta firmware for GALILEOSKY GLONASS/GPS v5.1, v5.0, v4.0, v2.5, v2.5 lite is added.

**Change log of 231.5 firmware:**

    Corrections:
    1) OBD error codes handling is fixed.
    2) Error in algorihms handling is fixed.

**Change log of 14 firmware:**

    New features:
    1) Archive on SD card.
    2) Archive uploading from SD card with every second detalization.
    3) A capability to control WiFi module from EasyLogic.
    4) Archive uploading from internal memory in chronological order.
    5) Wiegand26 support.
    Corrections:
    1) Spontaneous resets of terminal with WiFi module are fixed.

###4.12.26 (19.01.17)

**New features:**

- 229.14 stable firmware is added
- 230.14 beta firmware is added

**Change log of 229.14 and 230.14 firmwares:**

    Corrections:
    1) OBD error codes handling is fixed.
    2) Error in algorihms handling is fixed.

###4.12.25 (17.01.17)

**Corrections:**

- Remote connection to GALILEOSKY devices is fixed


###4.12.24 (29.12.16)

**New features:**

- 12.7 stable firmware for GALILEOSKY Base Block is added

**Change log of 12.7 firmware for GALILEOSKY Base Block:**

    Corrections:
    1) Spontaneous terminal reset is fixed.


###4.12.23 (27.12.16)

**Corrections:**

- Remote connection to GALILEOSKY v2.5 devices is fixed


###4.12.22 (26.12.16)

**New features:**

- 12.6 stable firmware for GALILEOSKY Base Block is added

**Change log of 12.6 firmware for GALILEOSKY Base Block:**

    Corrections:
    1) Fixed data transmission error in poor GSM coverage areas.


###4.12.21 (20.12.16)

**New features:**

- The ability to activate user defined OBD2 CAN filter for firmware 13 of GALILEOSKY Base Block is added.
- Built-in accelerometer's values are added into algorithms.


###4.12.20 (15.12.16) - Installer

**Corrections:**

- Internal memory download speed is optimized.
- Display of device state for GALILEOSKY Base Block is fixed.


###4.12.19 (08.12.16)

**Corrections:**

- Display of analog ins values for GALILEOSKY Base Block is fixed.


###4.12.18 (06.12.16)

**New features:**

- 229.13 stable firmware is added
- 13 beta-firmware of GALILEOSKY Base Block is added

**Change log of 229.13 firmware of GALILEOSKY terminals:**

    New features:
    1)  New command DELALLKEYS for deletion of all trusted keys from SD card is added.

**Change log of 13 beta-firmware of GALILEOSKY Base Block:**

    New features:
    1) GalileoSky photocamera support is added.


###4.12.17 (28.11.16)

**New features:**

- First firmware for GALILEOSKY BOXFINDER GSM with Iridium module is added


###4.12.15 (21.11.16)

**Corrections:**

- Display protocol settings page for GALILEOSKY v 4.0 and Base Block is fixed.


###4.12.14 (17.11.16)

**Corrections:**

- Display of parameters obtained via RS485 for GALILEOSKY v 4.0 is fixed.
- Display settings error for firmware with revision greater than 9 is fixed.
- Missing settings of RS485 operating mode for GALILEOSKY v4.0 and Base Block are added.


###4.12.13 (08.11.16)

**New features:**

- 229.12 stable firmware is added
- 230.13 beta-firmware is added

**Change log of 229.12 firmware of GALILEOSKY terminals:**

  Corrections:
  1)  External temperature sensors handling on DataCOLD500 is fixed

**Change log of 230.13 firmware of GALILEOSKY terminals:**

  Corrections:
  1) Connection behaviour in roaming for terminals with SIM800 is fixed. 
  2) External temperature sensors handling on DataCOLD500 is fixed 
	

###4.12.12 (28.10.16)

**Corrections:**

- Problem with protocol settings for GALILEOSKY Base Block lite is fixed


###4.12.11 (25.10.16)

**New features:**

- Support for GALILEOSKY Base Block 1.0.50 is added
- 12 beta-firmware of GALILEOSKY Base Block is added

**Changes:**

- Easy Logic: GALILEOSKY Button's event and action are removed

**Corrections:**

- iButton's tags(via RS485) were added into protocol for GALILEOSKY Base Block lite

**Change log of 12 beta-firmware of GALILEOSKY Base Block:**

    New features:
    1) BaseBlock v1.0.5 support.
    2) Long file names support in autoinformer.
	
    Corrections:
    1) Fixed wrong filtering of coordinates using ignition input.
    2) Fixed data transmission using EGTS protocol.


###4.12.10 (19.09.16)

**New features:**

- Support for GALILEOSKY BOXFINDER GSM is extended
- Easy Logic: Remove and rewrite algorithms from server are added
- 229.11 stable firmware is added
- 230.11 beta-firmware is added

**Change log of 229.11 and 230.11 firmwares of GALILEOSKY terminals:**

    Corrections:
    1) Fixed error in CAN-LOG data handling.
    2) Fixed return air handling from DataCOLD500.


###4.12.8 (08.09.16)

**Corrections:**

- 7 beta-firmware was removed, because it led to terminal’s malfunction in some cases


###4.12.7 (18.08.16)

**New features:**

- 10 beta-firmware of GALILEOSKY Base Block is added

**Change log of 10 beta-firmware of GALILEOSKY Base Block:**

    New features:
	1) BaseBlock Optimium, Hard and Wi-Fi support.
	2) Custom PID requests using J1979.
	3) CAN-LOG support using RS485.
	
	Corrections:
	1) The error of incoming SMS handler in algorithms is fixed

**Corrections:**

- Data downloading from internal flash memory for specified period is fixed
- The trouble of inability to accept SMS received from any telephone number for algorithms' block "Incoming SMS" is fixed


###4.12.6 (29.07.16)

**Corrections:**

- Operation via proxy server is corrected


###4.12.5 (11.07.16)

**New features:**

- Data downloading from internal flash memory for specified period is added


###4.12.4 (07.07.16)

**Corrections:**

- Fixed support for GALILEOSKY BOXFINDER SAT devices


###4.12.3 (06.07.16)

**New features:**

- 230.9 beta-firmware is added
- 7 beta-firmware of GALILEOSKY Base Block is added

**Change log of 230.9 beta-firmware of GALILEOSKY terminals:**

    Corrections:
    1) Fixed Trimble EzGuide compatibility.
    2) Fixed wrong sending order of photos.
	
**Change log of 7 beta-firmware of GALILEOSKY Base Block:**

    Corrections:
    1) Fixed wrong coordinates filtering.


###4.12.2 (24.06.16)

**New features:**

- 6 beta-firmware of GALILEOSKY Base Block is added

**Change log of 6 beta-firmware of GALILEOSKY Base Block:**

    Corrections:
	1) Fixed wrong coordinates filtering.


###4.12.1 (16.06.16)

**New features:**

- Support for GALILEOSKY BOXFINDER SAT devices is added

**Corrections:**

- Settings files of GALILEOSKY Base Block HARD WI-FI, HARD 3G and OPTIMUM is corrected


###4.12.0 (10.06.16)

**New features:**

- 5 beta-firmware of GALILEOSKY Base Block is added

**Change log of 5 beta-firmware of GALILEOSKY Base Block:**

    Corrections:
    1) Fixed wrong voltage measurement (first appeared in firmware 4).
    2) Fixed encoding of SMS with Russian language symbols.


###4.11.1 (09.06.16)

**New features**

- Small GUI changes for Windows 10 Touch Screen


###4.11.0 (08.06.16)

**New features:**

- Support for GALILEOSKY GPS v2.5 device is added
- 229.9 stable firmware is added
- 230.7 beta-firmware is added
- 4 beta-firmware of GALILEOSKY Base Block is added
- Representation of Iridium packet size of GALILEOSKY GPS/GLONASS Satellite v4.0 is added

**Improvements:**

- Reset settings to default is made by page. To reset all the settings, press and hold _Reset page_ button
- Speed up application startup

**Corrections:**

- Connection to remote server is corrected
- Online status of remote device is corrected

**Change log of 229.9 stable firmware of GALILEOSKY terminals:**

    New features:
    1) GALILEOSKY GLONASS/GPS v2.5 support.

**Change log of 230.7 beta-firmware of GALILEOSKY terminals:**

    New features:
    1) GALILEOSKY GLONASS/GPS v2.5 support.
    2) CAN-LOG support using RS485.

**Change log of 4 beta-firmware of GALILEOSKY Base Block:**

    Corrections:
    1) Fixed nulling of counted impulses after reset.


###4.10.0 (25.05.16)

**New features:**

- 3 beta-firmware for GALILEOSKY Base Block is added

**Corrections:**

- Fix downloading internal archive instead of external after reconnection

###4.9.4 (06.05.16)

**New features:**

- Tooltips for parameters on Settings page is added

**Corrections:**

- Flags representation on Protocol tab of Base Block LITE is corrected

###4.9.3 (27.04.16)

**Corrections:**

- GPS.CORRECT command representation - coordinates filtering

###4.9.2 (19.04.16)

**Corrections:**

- Show firmware selection dialog, if requested firmware file is not found

###4.9.1 (08.04.16)

**Corrections:**

- Minor enhancements

###4.9.0 (01.04.16)

**New features:**

- Support for GALILEOSKY GPS v2.4 lite device is added
- 229.8 stable firmware is added
- 230.6 beta-firmware is added

**New features of 229.8 and 230.6 firmware versions:**

- Support for GALILEOSKY GPS v2.4 lite devices is added

###4.8.1 (01.03.16)

**Corrections:**

- Added the ability to run more than one instance of Configurator on the same PC

###4.8.0 (17.02.16)

**New features:**

- 230.5 beta firmware is added

###4.7.0 (25.01.16)

**New features:**

- Support for GALILEOSKY BOXFINDER devices is added
- 4 beta-firmware for GALILEOSKY BOXFINDER devices is added

**Corrections:**

- Firmware change log is updated to 230.4 version

**GALILEOSKY BOXFINDER firmware change log:**

    [4_T_0000][22.01.2016]
        Corrections:
        1) Battery voltage determination error of GALILEOSKY BOXFINDER GSM v1.0 devices without socket is fixed.
        2) Unsealing sensor status setting is corrected.

    [3_T_0000][26.10.2015]
        New features:
        1) Support GALILEOSKY BOXFINDER GSM devices without socket.

    [1_T_0000][24.06.2015]
        New features:
        1) First release.

###4.6.1 (21.01.16)

**Corrections:**

- 229.7 stable firmware is updated

###4.6.0 (19.01.16)

**New features:**

- 229.7 stable firmware is added

###4.5.0 (25.12.15)

**Corrections:**

- Tag setting on CAN tab of Settings page is corrected

**New features:**

- Firmware change log is added to About dialog

###4.4.4 (19.12.15)

- Minimum default value of DFILTER command is corrected

###4.4.3 (15.12.15)

- 230.4 beta-firmware is corrected

###4.4.2 (14.12.15)

**Corrections:**

- Default maximum speed value in GPS.CORRECT command is corrected
- News and user manuals loading from official site is corrected
- Displaying of the device 3D-model when it is turned over is corrected
- Items titles on page Settings is corrected

**New features:**

- Language option icon is added

###4.4.1 (03.12.15)

**Corrections:**

- Displaying of device settings is corrected

###4.4.0 (26.11.15)

**New features:**

- Support for GALILEOSKY GPS/GLONASS v2.4 devices is added

**Changes:**

- Configurator contains following firmware versions:
    - 230.4 - beta-version;
    - 229.6 - stable;
    - 199 - stable;
    - 30 - stable (for old devices).

**Corrections:**

- Upgrade old devices to 30 firmware is corrected

**New features of 229.6 firmware:**

- GALILEOSKY GLONASS/GPS v2.4 support

**Corrections of 229.6 firmware:**

- Fixed CLEANPHOTOQUEUE command
- Fixed incorrect data recording in archive on SD card at 00:00 am
- Fixed GPRS session dropping after disconnection with server on terminals v5.1

###4.3.0 (20.11.15)

**New features:**

- 230 firmware support is added

**Corrections:**

- STATUS command processing is corrected
- DFILTER command processing for GALILEOSKY GPS/GLONASS v5.1 (3G) is corrected

**New features of 230 firmware:**

- Sending of additional data using EGTS protocol:
    - external power supply;
    - internal battery power;
    - status of inputs;
    - status of outputs;
    - analog inputs data;
    - digital fuel level sensors(FLS) data.
- Command for requesting CCID of active SIM-card
- Support of Trimble guidance systems on all devices with RS232 interface
- Maximum call time setting
- Command for setting mileage
- Filtering of RS485 FLS data
- Geofence count increased to 300
- Command for requesting active SIM-card's index and MNC/MCC of active GSM-network
- Setting to reset device if there are no sent data during specified interval

###4.2.5 (15.10.15) - Installer

- Upgrading of GALILEOSKY GPS/GLONASS v2.2.x devices to 199 firmware is fixed (was broken in version 4.2.1)

###4.2.4 (28.09.15)

- 229.4 firmware file is updated

###4.2.3 (09.09.15)

- Default ranges of powincfg command is corrected for GALILEOSKY GPS/GLONASS v5.0 devices

###4.2.2 (02.09.15)

- Default ranges of powincfg command is corrected

###4.2.1 (31.08.15)

- Firmware 229 is updated

###4.2.0 (21.08.15)

- Setting of the parameters on Protocol tab for 192-204 firmwares is corrected
- Choosing file for archive saving is corrected

###4.1.1 (31.07.15)

- GALILEOSKY GPS/ГЛОНАСС Satellite v4.0 settings is corrected

###4.1.0 (16.07.15)

- Operating with remote control server is improved
- Device upgrading procedure is unified

###4.0.5 (03.07.15)

Operation with device settings is changed:

- Device settings colorization is added:

    Color list according to priority order:
    1) _red_ - unknown parameter. Parameter value stored in device is unknown;
    2) _yellow_ - modified parameter. Value has been modified by user;
    3) _green_ - actual parameter. Parameter value has been loaded from device;

> Tab color is set to most priority color

- settings is loaded tab by tab:

    - loading setting of tab is initiated by switching on one;
    - to load all settings press and hold `Load tab` to open popup menu, than
        press `Load everything`;

- only modified parameters is going to be applied:

    - only _yellow_ parameters will be uploaded to device when `Apply` button
        is pressed

###4.0.4 (23.06.15)

- e-mail address for user registration is changed (support@7gis.ru)

###4.0.3 (01.06.15)

- 229-beta firmware file is updated

###4.0.2 (29.05.15)

- 229-beta firmware file is added
- Firmware upgrading is corrected

###4.0.1 (25.05.15) - Installer

- Firmware upgrading is corrected

###4.0.0 (12.05.15) - Installer

New features:

- Opportunity of the program operation without OpenGL drivers

Changes:

- The driver is set by a standalone installer as root
- Launch of the driver setting is carried out by a standard installer;
- The Configurator of version 4 is set in parallel with the Configurator of version 3

----------------------------------------------------------------------

###3.5.5 (27.04.15)

- Opportunity to choose �GALILEOSKY with compression� data transmission protocol is added starting from the firmware 229
- Table displaying is corrected on Protocol tab of Settings for the GPS/GLONASS Satellite v4.0 terminal.
- Sending of many network requests is corrected by the failed authorization on the proxy server

###3.5.3 (01.04.15)

- Absence the "use only SIM 1" option of the "SIMSwitch" command for GALILEOSKY GPS/GLONASS v5.0 devices is corrected
- Displaying of the outputs states on Ins/Outs tab is corrected
- "Max. speed" is removed, starting from firmware 228

###3.5.2 (18.03.15)

- Request for the OBD-II test confirmation is added
- Downloading of the internal archive (omission of a point and duplication of the next one) is corrected
- Maximum possible value of SPUTNIK command parameter is increased up to 2147483647
- Value of the first parameter of GPS.CORRECT2 command is increased up to 3600

###3.5.1 (13.02.15)

- Support of firmware 228 is added

###3.5.0 (29.12.14) - Installer

- Driver for GALILEOSKY devices is updated

###3.4.12 (11.12.14)

- Support of firmware 227 is added
- Files of firmware settings are corrected
- Installation of the Configurator is corrected if User Account Control (UAC) is enabled in Windows

###3.4.11 (01.12.14)

- Connection to device is corrected
- Displaying of the longitude on Routes tab is corrected

###3.4.10 (14.11.14)

- Support of firmware 226 corrections is added
- Opportunity of choosing all registers on CAN tab of Settings page is corrected.
- CAN scanning for the remote devices is corrected.
- Geofences saving to the local device is corrected.
- Device registration on the remote server by having zeroes at the beginning of IMEI is corrected.

###3.4.9 (03.10.14)

- Support of the GALILEOSKY GPS/GLONASS v5.1 device (3G, SIM-chip) is fixed

###3.4.8 (09.09.14)

- Support of the GALILEOSKY GPS/GLONASS v5.1 device (3G, SIM-chip) is added
- Support of firmware 226 is added

###3.4.7 (01.09.14)

- Geofences setting by the configuring of remote device is corrected
- Setting of digital inputs for the GALILEOSKY v2.3 lite device is corrected
- CAN data display on Device tab for the GALILEOSKY v2.3 lite device is corrected

###3.4.6 (01.08.14) - Installer

- Geofences download from the device and from settings file is corrected
- Description of Galileo protocol parameters is corrected
- Troubleshooting points are renamed

###3.4.5 (21.07.14)

- Accelerometer troubleshooting is added to GALILEOSKY v1.8.5 lite and GALILEOSKY v2.3 lite devices
- Connection to devices via USB is corrected

###3.4.4 (02.07.14)

- Support of firmware 224 is added
- Data transmission from a CSV-file to the server is corrected
- Commands forming of the list of cellular operators codes and FLS calibration tables is corrected

###3.4.3 (25.06.14)

- Archive download for the GALILEOSKY v1.8.5 lite devices is fixed
- Firmware upgrade for the obsolete devices is fixed

### 3.4.2 (18.06.14) - Installer

- Opportunity to upgrade firmware of the GALILEOSKY GPS/GLONASS Satellite v4.0 device is added

- Storing of the folder, from which the file of the device settings is opened, is corrected
- Storing of log files and program settings by the Configurator updating is corrected

### 3.4.1 (06.06.14)

- The Tenzo-M weight indicator function of the RS-232 port is added
- The AWT640 weight indicator function of the RS-232 port is added
- The Test RS232 function of the RS-232 port is added
- The height field is added on the Device tab
- Firmware 223 for the GALILEOSKY GPS v2.3 lite device is added

- Download of the internal archive for firmwares 205 and further is corrected

### 3.4.0 (19.05.14) - Installer

- Support of firmware 223 (EGTS protocol) is added
- Options of archive structure control for the GALILEOSKY GPS vX. X lite devices are added
- Boot loader is corrected. The updating of the Configurator is carried out even if the current version is installed
- Data sending to the server is corrected
- The structure size of the refrigerator by calculating the size of the point, sent to the server, is corrected
- The structure size of the refrigerator by the uploading from the internal archive is corrected

### 3.3.2 (13.05.14)

- Firmware upgrade for the GPS/GLONASS v5.1 (3G) and GPS/GLONASS Satellite v4.0 devices is supported

### 3.3.1 (19.02.14) - Installer

- Updating for some parameters is added on the Protocol tab, so they can be stored only in dynamic archive
- The Refrigerator parameter is added on the Protocol tab
- The Upgrade firmware button is not displayed for the GPS/GLONASS Satellite v4.0 device

### 3.3.0 (05.02.14) - Installer

- Automatic update of the Configurator is implemented
- Support of the device 21 (v5.1) is added, starting from firmware 207
- Displaying of the point size, sent to the server, is added by choosing the archive location on microSD
- Support of the REMOTECONFIG command is added for the lite devices
- The Driving field in the Navigation data group is added on the Device tab. The Acceleration by... field is deleted from the Analog inputs group
- The Satellite modem option is added on the Troubleshooting tab
- Processing of the negative temperature in the reply of the RS485 command is corrected
- Calculation of points number in static archive is corrected
- Calculation of points size is corrected. Point size is calculated for data transmission via a satellite
- Operation with a proxy server is corrected

### 3.2.10

- Displaying of a track from CSV-file is corrected
- Data storage from the device internal memory is corrected

### 3.2.9

- Editing of the codes list for cellular operators is improved
- Support of firmware 221 is added

### 3.2.8

- Support of the 1.9-lite devices is corrected

### 3.2.7

- Displaying of the device type is added on the Device tab
- Work with the CAN troubleshooting section is improved
- Support of firmware 206: DBG-S11D dosimeter, the "Not clear data after the CAN-bus disconnection" option
- Support of firmware 199: the "Not clear data after the CAN-bus disconnection" option

### 3.2.6

- Maximum length of the authorized phone number - 14 symbols
- Displaying of news from web-site is corrected
- Support of firmware 220 is added
- Support of the technological firmware by the 1.9, 1.9-lite, 2.3 devices is corrected

### 3.2.5

- Download speed of the devices list by remote configuring is increased dramatically

### 3.2.4

- Support of firmware 204 is added

### 3.2.3

- Timeout determination from the CANREGIME command is corrected
- Calculation of the size of the records, stored in the archive and sent to the server, is corrected
- Corrected: there is no RS232, only RS485 in device 16

### 3.2.2

- Displaying of the record size of one point, sent to the server, is added
- Loss of some troubleshooting messages is corrected
- Support of firmware 199 is corrected

### 3.2.1

- Support of firmware 210 is added

### 3.2.0

- Support of the 2.3, 1.9, 1.9 lite devices is added
- Support of firmwares 201 and 202 is added

### 3.1.9

- Upload of the archive from SD-card is corrected
- By default the Routes  tab centers on the coordinates of the connected device

### 3.1.8

- Correction of firmware 200
- Connection via a proxy server is corrected

### 3.1.7

- Support of firmware 200 is added
- Error of the firmware upgrade from zip-file from a disc is corrected
- Correction of the connection to a proxy server
- Loading of the Internet channel is decreased by connection to the remote server

### 3.1.5

- Opportunity to specify a proxy server via the parameter of the command line is added:

        -proxy <host>: <port>: <user>: <password>

- Support of old devices is corrected

### 3.1.4

- Opportunity to register the list of devices is added
- Indicator of commands processing by the remote server is added to the dialog of device choice
- Processing of the commands, sent to the remote server, is corrected
- Loading of the Internet channel is decreased at the moment of connection to the remote server

### 3.1.3

- Support of old devices is corrected

### 3.1.2

- Disconnection of the Configurator from the server is corrected by a big number of the user's devices
- Deleting of devices group is carried out after the action confirmation
- Download speed  of the commands list is increased
- Descriptions of i-Button actions are specified: trusted key or any other key

### 3.1.1

- Read error of archive configuration settings is corrected

### 3.1.0

- ...
- Support of RS485[0..2] parameters sending to the server from CSV-file is added
- Dialog of the user registration is improved

### 3.0.7

- Support of firmware 193 is added
- Support of the headpack2, mainpack2 commands is added to firmware 186
- Downloading of the English documentation from website is added

### 3.0.6

- The User's Manual for GalileoSky GPS\GLONASS v5.0 terminals (firmware 0192) is updated
- Opportunity to download the missing documentation from web-site (GalileoSky GPS\GLONASS, GalileoSky GPS lite)
- Support of firmwares 191 and 192 is added
- Opportunity to send commands in the command mode for the remote device in line is added
- Support of the headpack2, mainpack2 commands (starting from firmware 190) is added
- Support of the remoteconfig command (starting from firmware 186) is added
- CAN scanning for the remote device is corrected
- The use of system proxy is corrected

### 3.0.5

- Opportunity to store the results of the CAN reading to the file and reading them from this file
- Commands for the control of the internal archive structure are added
- Displaying of points number by the dynamic structure of the internal archive is added

### 3.0.4

- Archive upload from the device with beta-firmwares is corrected
- Troubleshooting for all firmwares of all devices is corrected

### 3.0.3

- Support of firmware 184

#### 3.0.2

- Error of the displaying of the device 3D-model is corrected

### 3.0.1

- Debugging messages of the operation with the remote device are added to the log file
- Displaying of the process of the remote device state scanning is added
- Displaying of the remote devices as inactive in the list by choosing the remote device commutator is corrected
- Width of the setting field, not containing the text, displayed by default, is corrected
- Search for the device driver in the system catalog is corrected
- Error, arising by the program close down, is corrected
- Error, not allowing to reconnect to the device, is corrected
- Reactivation of the remote device troubleshooting after its miss is corrected

### 3.0.0

- Program interface is changed
- 3D-model of the device is changed
- Request for changing the password by the remote device registration
- Reading of the authorized phones from file for all devices is corrected
